DOCUMENT 01 76 00

ALTERATION PROJECT PROCEDURES

1. – GENERAL
	1. RELATED DOCUMENTS AND PROVISIONS:

All Contract Documents should be reviewed for applicable provisions related to the provisions in this document, including without limitation:

* + 1. General Conditions, including, without limitation, Integration of Work, Purchase of Materials and Equipment, Uncovering of Work and Non-conforming Work and Correction of Work and Trenches;
		2. Special Conditions.
1. - PRODUCTS
	1. PRODUCTS FOR PATCHING AND EXTENDING WORK:
		1. New Materials: As specified in the Contract Documents including, without limitation, in the Specifications, Contractor shall match existing products, conditions, and work for patching and extending work.
		2. Type and Quality of Existing Products: Contractor shall determine by inspection, by testing products where necessary, by referring to existing conditions and to the Work as a standard.
2. - EXECUTION
	1. EXAMINATION:
		1. Contractor shall verify that demolition is complete and that areas are ready for installation of new Work.
		2. By beginning restoration Work, Contractor acknowledges and accepts the existing conditions.
	2. PREPARATION:
		1. Contractor shall cut, move, or remove items as necessary for access to alterations and renovation Work. Contractor shall replace and restore these at completion.
		2. Contractor shall remove unsuitable material not as salvage unless otherwise indicated in the Contract Documents. Unsuitable material may include, without limitation, rotted wood, corroded metals, and deteriorated masonry and concrete. Contractor shall replace materials as specified for finished Work.
		3. Contractor shall remove debris and abandoned items from all areas of the Site and from concealed spaces.
		4. Contractor shall prepare surface and remove surface finishes to provide for proper installation of new Work and finishes.
		5. Contractor shall close openings in exterior surfaces to protect existing work from weather and extremes of temperature and humidity. Contractor shall insulate ductwork and piping to prevent condensation in exposed areas. Contractor shall insulate building cavities for thermal and/or acoustical protection, as detailed.
	3. INSTALLATION:
		1. Contractor shall coordinate Work of all alternations and renovations to expedite completion and to accommodate District occupancy.
		2. Designated Areas and Finishes: Contractor shall complete all installations in all respects, including operational, mechanical work and electrical work.
		3. Contractor shall remove, cut, and patch Work in a manner to minimize damage and to provide a means of restoring Products and finishes to original or specified condition.
		4. Contractor shall refinish visible existing surfaces to remain in renovated rooms and spaces, to specified condition for each material, with a neat and square or straight transition to adjacent finishes.
		5. Contractor shall install products as specified in the Contract Documents, including without limitation, the Specifications.
	4. TRANSITIONS:
		1. Where new Work abuts or aligns with existing, Contractor shall perform a smooth and even transition. Patched Work must match existing adjacent work in texture and appearance.
		2. When finished surfaces are cut so that a smooth transition with new Work is not possible, Contractor shall terminate existing surface along a straight line at a natural line of division and make a recommendation for resolution to the District and the Architect for review and approval.
	5. ADJUSTMENTS:
		1. Where removal of partitions or walls results in adjacent spaces becoming one, Contractor shall rework floors, walls, and ceilings to a smooth plane without breaks, steps, or bulkheads.
		2. Where a change of plane of 1/4 inch or more occurs, Contractor shall submit a recommendation for providing a smooth transition to the District and the Architect for review and approval.
		3. Contractor shall trim and seal existing wood doors and shall trim and paint metal doors as necessary to clear new floor finish and refinish trim as required.
		4. Contractor shall fit Work at penetrations of surfaces.
	6. REPAIR OF DAMAGED SURFACES:
		1. Contractor shall patch or replace portions of existing surfaces, which are damaged, lifted, discolored, or showing other imperfections, in the area where the Work is performed.
		2. Contractor shall repair substrate prior to patching finish.
	7. CULTIVATED AREAS AND OTHER SURFACE IMPROVEMENTS:
		1. Cultivated or planted areas and other surface improvements which are damaged by actions of the Contractor shall be restored by Contractor to their original condition or better, where indicated.
		2. Contractor shall protect and replace, if damaged, all existing guard posts, barricades, and fences.
		3. Contractor shall give special attention to avoid damaging or killing trees, bushes and/or shrubs on the Premises and/or identified in the Contract Documents, including without limitation, the Drawings.
	8. FINISHES:
		1. Contractor shall finish surfaces as specified in the Contract Documents, including without limitations, the provisions of all Divisions of the Specifications.
		2. Contractor shall finish patches to produce uniform finish and texture over entire area. When finish cannot be matched, Contractor shall refinish entire surface to nearest intersections.
	9. CLEANING:
		1. Contractor shall continually clean the Site and the Premises as indicated in the Contract Documents, including without limitation, the provisions in the General Conditions and the Specifications regarding cleaning.

END OF DOCUMENT